**The experimental research of cyclotron DC-280 work**

V.A. Semin\*, I.V. Kalagin, A.A. Protasov, V.I. Mironov, D.K. Pugachev, P.I. Vinogradov

*Joint Institute for Nuclear Research Flerov laboratory of nuclear reaction*

\*E-mail: seminva@jinr.ru

The DC280 is the high current cyclotron with design beam intensities up to 10 pμA for ions with energy from 4 to 8 MeV/nucleon. It was developed and created at the FLNR JINR. The first was extracted from the cyclotron on January 17, 2019. Experiments on acceleration of 84Kr, 12C, 40Ar, 48Ca, 48Ti, 52Cr and 54Cr beams production were carried out. The following intensities of accelerated beam have been achieved: 1.43 pμA for 84Kr+14; 10 pμA for 12C+2; 9,2 pμA for 40Ar+7; 7,7 pμA for 48Ca+7. The long time experiments were done in 2020-2022. The features of work of High Voltage axial injection systems, buncher systems and Flat-top systems were explored. The work of accelerator was stable and high efficiency. The total acceleration efficiency from ion source to transport channel was about 46%.

1. B.N. Gikal *et al.,* ”Start-Up of the DC-280 Cyclotron, the Basic Facility of the Factory of Super heavy Elements of the Laboratory of Nuclear Reactions at the Joint Institute for Nuclear Research”, *ISSN 1814-5957, Nuclear Research Physics of Particles and Nuclei Letters,*Vol. 16, p.866-875 2019.DOI:[10.1134/S1547477119060177](http://dx.doi.org/10.1134/S1547477119060177)
2. V.A. Semin *et al.,* “DC-280 cyclotron for Factory of Super Heavy Elements experimental results.” *In Proc. of 12th Int. Particle Acc. Conf. (IPAC2021)* p.p. 4126-4129, 2021.

doi:10.18429/JACoW-IPAC2021-THPAB182

1. V.A. Semin et al., “The experimental research of cyclotron DC-280 beam parameter”, presented at the 27th Russian Particle Acc. Conf. (RuPAC2021), Alushta, Russia, October, paper FRA04. ISSN: 2673-5539

doi:10.18429/JACoW-RuPAC2021-FRA04

https://accelconf.web.cern.ch/rupac2021/papers/FRA04.pdf