**Determination of neutron detection efficiency of DEMON and PARIS detectors using a 252Cf source**

O. Saiko1,2, E.M. Kozulin1,2, K. Kulkov1,2, K.V. Novikov1,2,

Yu.E. Penionzhkevich2,3, Yu.G. Sobolev2, S.S. Stukalov2,

I.V. Vorobiev2, Zh. Zeinulla2,4

*1Dubna State University, Dubna, Russia;*

 *2Flerov Laboratory of Nuclear Reactions, Joint Institute for Nuclear Research,*

*Dubna, Russia;*

*3Department of Experimental Methods in Nuclear Physics, National Research Nuclear University, Moscow, Russia*

*4Institute of Nuclear Physics, Almaty, Kazakhstan;*

 E-mail: saiko@jinr.ru

The results of measuring the energy distribution of neutrons emitted from the 252Cf source by the DEMON and PARIS detectors are presented. DEMON (DEtecteur MOdulaire de Neutrons) is scintillator detector widely used for neutron detection [1]. PARIS (Photon Array for the studies with Radioactive Ion and Stable beams) is new-built detector consisting of CeBr3 - NaI(Tl) phoswich scintillators [2].

The energies of the neutrons were measured by the Time – Of – Flight (TOF) method where a semiconductor detector was used for fission fragment detection and START-pulse generation for the TOF measurements. The STOP pulses for TOF measurements were generated by DEMON and PARIS detectors, respectively.

The energy dependence of the neutron efficiency for DEMON and PARIS detectors at the *E*n = 0.7 ÷ 7 MeV neutron energy range were determined by comparing the measured data with standard 252Cf spectrum [3].

1. I. Tilquin et al., Nucl. Instr. Meth. A 365, 446 (1995).

2. A. Maj et al., Acta Phys. Pol. B 40, 565 (2009).

3. W. Mannhart, Proc. of IAEA Consulting Meeting*,* INDC(NDS)-220, p. 305 (1989).